BiCom System

A BiCom system is the extention of the unidirectional RKE to bidirectional RKE system.

* keyfob -> car (like a unidirectional RKE system)
* car -> keyfob (car status information for displaying on the keyfob by LED or display

Typical BiCom status information transmitted to the keyfob are:

* Window status :- ( switch on- All led on at the same time)
* Alarm status - (Press switch two times- All led off at the same time
* Car battery info – (Press switch three times- All led on in clockwise manner)
* Door status (Press switch four times- All led on in anti-clockwise manner)